

1. Connect capture device with the PC or laptop with a USB cable.  
2. Open the PRO-CaptureSDI FW010819-1 folder.  
3. Double click the file named "01.Burn\_HW\_FW\_DESC.bat"

4. CMD window will pop out automatically  
5. The update process is successful If you can see the green words (Burn Pass) in below 2 places



6. Un-plug and re-connect the USB capture with your PC and HDMI source.